# Class CIM_MPLSCRLSPTrfcProf
extends CIM_MPLSQosPRTrfcProf

Class to represent the Constraint-based Routed LSP (CR-LSP) traffic parameters as specified in [RFC3212].

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_MPLSQosPRTrfcProf
|
+--CIM_MPLSCRLSPTrfcProf

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Class to represent the Constraint-based Routed LSP (CR-LSP) traffic parameters as specified in [RFC3212].
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::MPLS
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CRLSPCommitedBurstSize | uint16 |
Description | string | Property to indicate the CR-LSP's committed burst size in bytes.
PUnit | string | byte
Units | string | Bytes
CRLSPCommitedDataRate | uint16 |
Description | string | Property to indicate the CR-LSP's committed data rate in bytes per second.
PUnit | string | byte / second
Units | string | Bytes per Second
CRLSPFrequency | uint16 |
Description | string | Property to indicate at what granularity the CDR (allocated to the CR-LSP) is made available.
ValueMap | string | 0, 1, 2
Values | string | Unspecified, Frequently, Very Frequently
CRLSPWeight | uint8 |
Description | string | Property to indicate the CR-LSP's relative share (in percent) of the possible excess bandwidth above its committed rate.
MaxValue | sint64 | 100
MinValue | sint64 | 0
PUnit | string | percent
Units | string | Percent

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
PRExcessBurst | uint16 | CIM_MPLSQosPRTrfcProf
PRNormalBurst | uint16 | CIM_MPLSQosPRTrfcProf
PRRate | uint32 | CIM_MPLSQosPRTrfcProf

## Class Methods