# Class CIM_LLDPEthernetPortStatistics
extends CIM_EthernetPortStatistics

This class describes LLDP statistics that applies to LLDP frames on this Ethernet Port. For more detailed descriptions on these properties, please refer to IEEE LLDP-EXT-DOT1-V2-MIB.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_NetworkPortStatistics
|
+--CIM_EthernetPortStatistics
|
+--CIM_LLDPEthernetPortStatistics

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class describes LLDP statistics that applies to LLDP frames on this Ethernet Port. For more detailed descriptions on these properties, please refer to IEEE LLDP-EXT-DOT1-V2-MIB.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.34.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
RxDestMACAddress | string[] |
ArrayType | string | Indexed
Description | string | The remote MAC addresses from which LLDP frames were received through the port to which these statistics apply.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsRxDestMACAddress
RxPortAgeoutsTotal | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | The number of age-outs in the (remote) port of the remote MAC address in the corresponding entry of RxDestMACAddress. This array and the RxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsRxPortAgeoutsTotal
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.RxDestMACAddress
RxPortFramesDiscardedTotal | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | he number of LLDP frames received through the port to which these statistics apply from the remote MAC address in the corresponding entry of RxDestMACAddress, that were then discarded for any reason. This array and the RxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsRxPortFramesDiscardedTotal
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.RxDestMACAddress
RxPortFramesErrors | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | The number of LLDP frames with errors received through the port to which these statistics apply from the remote MAC address in the corresponding entry of RxDestMACAddress. This array and the RxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsRxPortFramesTotal
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.RxDestMACAddress
RxPortTLVsDiscardedTotal | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | The number of TLVs in LLDP frames received through the port to which these statistics apply from the remote MAC address in the corresponding entry of RxDestMACAddress, that were discarded for any reason. This array and the RxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsRxPortTLVsDiscardedTotal
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.RxDestMACAddress
RxPortTLVsUnrecognizedTotal | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | The number of TLVs in LLDP frames received through the port to which these statistics apply from the remote MAC address in the corresponding entry of RxDestMACAddress, that were not recognized. This array and the RxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsRxPortTLVsUnrecognizedTotal
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.RxDestMACAddress
TxDestMACAddress | string[] |
ArrayType | string | Indexed
Description | string | The remote MAC addresses to which LLDP frames were transmitted through the port to which these statistics apply.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsTxDestMACAddress
TxLLDPDULengthErrors | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | The number of LLDPDU Length Errors recorded for the LLDP frames transmitted through this port to which these statistics apply to the remote MAC address in the corresponding entry of TxDestMACAddress. This array and the TxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsTxLLDPDULengthErrors
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.TxDestMACAddress
TxPortFramesTotal | uint32[] |
ArrayType | string | Indexed
Counter | boolean | true
Description | string | The number of LLDP frames transmitted through the port to which these statistics apply to the remote MAC address in the corresponding entry of TxDestMACAddress. This array and the TxDestMACAddress array shall be index-correlated.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2StatsTxPortFramesTotal
ModelCorrespondence | string | CIM_LLDPEthernetPortStatistics.TxDestMACAddress

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AlignmentErrors | uint32 | CIM_EthernetPortStatistics
BytesReceived | uint64 | CIM_NetworkPortStatistics
BytesTransmitted | uint64 | CIM_NetworkPortStatistics
Caption | string | CIM_ManagedElement
CarrierSenseErrors | uint32 | CIM_EthernetPortStatistics
DeferredTransmissions | uint32 | CIM_EthernetPortStatistics
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
ExcessiveCollisions | uint32 | CIM_EthernetPortStatistics
FCSErrors | uint32 | CIM_EthernetPortStatistics
FrameTooLongs | uint32 | CIM_EthernetPortStatistics
InstanceID | string | CIM_StatisticalData
InternalMACReceiveErrors | uint32 | CIM_EthernetPortStatistics
InternalMACTransmitErrors | uint32 | CIM_EthernetPortStatistics
LateCollisions | uint32 | CIM_EthernetPortStatistics
MultipleCollisionFrames | uint32 | CIM_EthernetPortStatistics
PacketsReceived | uint64 | CIM_EthernetPortStatistics
PacketsTransmitted | uint64 | CIM_EthernetPortStatistics
SampleInterval | datetime | CIM_StatisticalData
SingleCollisionFrames | uint32 | CIM_EthernetPortStatistics
SQETestErrors | uint32 | CIM_EthernetPortStatistics
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData
SymbolErrors | uint32 | CIM_EthernetPortStatistics

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData