# Class CIM_iSCSICapabilities
extends CIM_Capabilities

The capabilites for an iSCSI Network Entity. An instance of this class will be associated by ElementCapabilities to a instance of ComputerSystem that represents the Network Entity. These capability properties are associated to a Network Entity/ComputerSystem since they affect all login negotiations on all iSCSI ProtocolEndpoints aggregated to the system.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_iSCSICapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The capabilites for an iSCSI Network Entity. An instance of this class will be associated by ElementCapabilities to a instance of ComputerSystem that represents the Network Entity. These capability properties are associated to a Network Entity/ComputerSystem since they affect all login negotiations on all iSCSI ProtocolEndpoints aggregated to the system.
UMLPackagePath | string | CIM::Network::iSCSI
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaximumSpecificationVersionSupported | uint8 |
Description | string | The maximum version number of the iSCSI specification such that this iSCSI instance supports this maximum value, the minimum value indicated by the corresponding property MinimumSpecificationVersionSupported, and all versions in between.
MappingStrings | string | MIB.IETF|ISCSI-MIB.iscsiInstVersionMax
MaxValue | sint64 | 255
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_iSCSICapabilities.MinimumSpecificationVersionSupported, CIM_iSCSIConnection.ActiveiSCSIVersion
MinimumSpecificationVersionSupported | uint8 |
Description | string | The minimum version number of the iSCSI specification such that this iSCSI instance supports this minimum value, the maximum value indicated by the corresponding property MaximumSpecificationVersionSupported, and all versions in between.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiInstVersionMin
MaxValue | sint64 | 255
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_iSCSICapabilities.MaximumSpecificationVersionSupported, CIM_iSCSIConnection.ActiveiSCSIVersion
AuthenticationMethodsSupported | uint16[] |
ArrayType | string | Indexed
Description | string | An array containing a list of authentication methods supported by this Network Entity.
MappingStrings | string | MIB.IETF|IPS-AUTH-MIB.ipsAuthCredAuthMethod
ModelCorrespondence | string | CIM_iSCSIConnectionSettings.PrimaryAuthenticationMethod, CIM_iSCSIConnectionSettings.SecondaryAuthenticationMethod, CIM_iSCSIConnection.AuthenticationMethodUsed
ValueMap | string | 2, 3, 4, 5
Values | string | (None, SRP, CHAP, Kerberos
OtherSupportedFeatures | string[] |
Description | string | A string describing the additional supported features of the Network Entity, used when the corresponding SupportedFeatures array element is set to the value "1" (Other). Each element that corresponds to a SupportedFeatures array element with a value other than "1" (Other) shall have a value of NULL.
ModelCorrespondence | string | CIM_iSCSICapabilities.SupportedFeatures
SupportedFeatures | uint16[] |
Description | string | An enumeration indicating features that are supported by the Network Entity. Since this is an array, multiple values may be specified. The current values in the enumeration are: 0 = "None", indicating that no features are supported. If this value is present in the array, it shall be the only value. 1 = "Other", indicating that a feature not described by another value is present. A description of the capability can be found in the OtherSupportedFeatures property. "Other" can be present more than once in the SupportedFeatures array. 2 = "iSCSI Session", indication that the Network Entity supports iSCSI sessions.
ValueMap | string | 0, 1, 2
Values | string | None, Other, iSCSI Session

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities