# Class CIM_FCTopologyView
extends CIM_View

The CIM_TopologyView provides the properties to be able to build a topology without having to do associators from the ProtocolEndpoint to the FCPort to the FCNode or FCSwitch.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_View
|
+--CIM_FCTopologyView

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The CIM_TopologyView provides the properties to be able to build a topology without having to do associators from the ProtocolEndpoint to the FCPort to the FCNode or FCSwitch.
UMLPackagePath | string | CIM::Device::Views
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AntecedentElementWWN | string |
Description | string | The FC Switch Name Identifier (FC Switch WWN) or FC Node Name (FC Node WNN) the AntecedentFCPort is associated to.
AntecedentFCPort | string |
Description | string | The antecedent FCPort that is communicating with the dependent FCPort.
Reference | string | CIM_FCPort
AntecedentFCPortElementName | string |
Description | string | The user friendly name of the FCPort the antecedent reference is associated to.
AntecedentFCPortType | uint16 |
Description | string | The PortType of the FCPort the dependent reference is associated to.
AntecedentFCPortWWN | string |
Description | string | The FC Port Name Identifier (FC Port WWN) of the FCPort the antecedent reference is associated to.
AntecedentSystem | string |
Description | string | The System of the antecedent FCPort in the AntecedentFCPort SystemDevice association.
Reference | string | CIM_System
DependentElementWWN | string |
Description | string | The FC Switch Name Identifier (FC Switch WWN) or FC Node Name (FC Node WNN) the DependentFCPort is associated to.
DependentFCPort | string |
Description | string | The dependent FCPort that is communicating with the antecedent FCPort.
Reference | string | CIM_FCPort
DependentFCPortElementName | string |
Description | string | The user friendly name of the FCPort the dependent reference is associated to.
DependentFCPortType | uint16 |
Description | string | The PortType of the FCPort the dependent reference is associated to.
DependentFCPortWWN | string |
Description | string | The FC Port Name Identifier (FC Port WWN) of the FCPort the dependent reference is associated to.
DependentSystem | string |
Description | string | The System of the dependent FCPort in the DependentFCPort SystemDevice association.
Reference | string | CIM_System
InstanceID | string |
Description | string | Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. To ensure uniqueness within the NameSpace, the value of InstanceID should be constructed using the following 'preferred' algorithm: <OrgID>:<LocalID> Where <OrgID> and <LocalID> are separated by a colon ':', and where <OrgID> must include a unique name. It can be a copyrighted, trademarked, or otherwise unique name that is owned by the business entity that is creating or defining the InstanceID. Or, it could be a registered ID that is assigned to the business entity by a recognized global authority.(This requirement is similar to the <Schema Name>_<Class Name>> structure of Schema class names.) In addition, to ensure uniqueness <OrgID> must not contain a colon (':'). When using this algorithm, the first colon to appear in InstanceID must appear between <OrgID> and <LocalID>. <LocalID> is chosen by the business entity and should not be re-used to identify different underlying (real-world) elements. If the above 'preferred' algorithm is not used, the defining entity must ensure that the resulting InstanceID is not re-used as any of InstanceIDs produced by this or other providers for the NameSpace of this instance. For DMTF-defined instances, the 'preferred' algorithm must be used with the <OrgID> set to 'CIM'.
Key | boolean | true
Override | string | InstanceID

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement

## Class Methods