# Class CIM_EFService
extends CIM_DiffServService

This class represents a specialization of the general concept of forwarding network traffic by adding specific semantics that characterize the operation of the Expedited Forwarding (EF) Service (defined in RFC 2598). The EF PHB can be used to build a low loss, low latency, low jitter, assured bandwidth, end-to-end service through DiffServ domains. Such a service appears to the endpoints like a point-to-point connection or a virtual leased line. This service has also been described as Premium service in the IETF literature. RFC 2598 defines one DSCP for the EF service. Thus, there is no need to define any attributes in this class, since an instance of the EFService class, by definition, means that this particular DSCP is used. EFService is deprecated since forwarding based on the value of the DiffServ Code Point is specified using a FilterList, which is associated with a ClassifierElement. If there is a need to distinguish a higher-level set of coordinated QoS services, the DiffServService class can be instantiated directly.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_QoSService
|
+--CIM_DiffServService
|
+--CIM_EFService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_DiffServService
Description | string | This class represents a specialization of the general concept of forwarding network traffic by adding specific semantics that characterize the operation of the Expedited Forwarding (EF) Service (defined in RFC 2598). The EF PHB can be used to build a low loss, low latency, low jitter, assured bandwidth, end-to-end service through DiffServ domains. Such a service appears to the endpoints like a point-to-point connection or a virtual leased line. This service has also been described as Premium service in the IETF literature. RFC 2598 defines one DSCP for the EF service. Thus, there is no need to define any attributes in this class, since an instance of the EFService class, by definition, means that this particular DSCP is used. EFService is deprecated since forwarding based on the value of the DiffServ Code Point is specified using a FilterList, which is associated with a ClassifierElement. If there is a need to distinguish a higher-level set of coordinated QoS services, the DiffServService class can be instantiated directly.
UMLPackagePath | string | CIM::Network::QoS
Version | string | 2.7.0

## Class Properties

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DSCP | uint8 | CIM_DiffServService
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PHBID | uint16 | CIM_DiffServService
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service