# Class CIM_MemoryMappedIO
extends CIM_SystemResource

Personal Computer architecture Memory Mapped I/O. This class addresses both memory and port I/O resources. The property, MappedResource, defines whether memory or I/O is mapped (and for I/O whether the mapping is to a memory or a port space).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_SystemResource
|
+--CIM_MemoryMappedIO

## Direct Known Subclasses

CIM_MemoryResource
CIM_PortResource

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Personal Computer architecture Memory Mapped I/O. This class addresses both memory and port I/O resources. The property, MappedResource, defines whether memory or I/O is mapped (and for I/O whether the mapping is to a memory or a port space).
UMLPackagePath | string | CIM::System::SystemResources
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CreationClassName | string |
Description | string | CreationClassName indicates the name of the class or the subclass used in the creation of an instance. When used with the other key properties of this class, this property allows all instances of this class and its subclasses to be uniquely identified.
Key | boolean | true
MaxLen | uint32 | 256
CSCreationClassName | string |
Description | string | The scoping ComputerSystem's CreationClassName.
Key | boolean | true
MaxLen | uint32 | 256
Propagated | string | CIM_ComputerSystem.CreationClassName
CSName | string |
Description | string | The scoping ComputerSystem's Name.
Key | boolean | true
MaxLen | uint32 | 256
Propagated | string | CIM_ComputerSystem.Name
EndingAddress | uint64 |
Description | string | Ending address of memory mapped I/O.
MappingStrings | string | MIF.DMTF|Memory Mapped I/O|001.2
MappedResource | uint16 |
Description | string | Type of memory mapped I/O. MappedResource defines whether memory or I/O is mapped, and for I/O, whether the mapping is to a memory or a port space.
ValueMap | string | 0, 1, 2, 3
Values | string | Other, Mapped Memory, I/O Mapped to Memory Space, I/O Mapped to Port Space
StartingAddress | uint64 |
Description | string | A part of the object's key value, the starting address of memory mapped I/O.
Key | boolean | true
MappingStrings | string | MIF.DMTF|Memory Mapped I/O|001.1

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
ImplementationInfo | uint16 | CIM_SystemResource
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Shareable | boolean | CIM_SystemResource
Status | string | CIM_ManagedSystemElement
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
RequestStateChange | uint32 | CIM_EnabledLogicalElement