# Class CIM_PersistentMemoryNamespaceSettingData
extends CIM_ResourceAllocationSettingData

PersistentMemoryNamespaceSettingData reflects the parameters specified during persistent memory namespace creation or modification that define the quality of service offered by the associated PersistentMemoryNamespace.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_ResourceAllocationSettingData
|
+--CIM_PersistentMemoryNamespaceSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | PersistentMemoryNamespaceSettingData reflects the parameters specified during persistent memory namespace creation or modification that define the quality of service offered by the associated PersistentMemoryNamespace.
UMLPackagePath | string | CIM::Device::ConfigurableMemory
Version | string | 2.47.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AccessType | uint16 |
Description | string | The type of access supported for the namespace."Read" read access is supported. "Write" write access is supported. "Read/Write" read and write access is supported.
ValueMap | string | 0, 2, 3, 4, .., 0x8000..0xFFFF
Values | string | Unknown, Read, Write, Read/Write, DMTF reserved, Vendor Reserved
Optimize | uint16 |
Description | string | Describes preferences relating to the allocation that can be described by flags "None" no specific optimizations requested. "Best Performance" Namespace optimized for best performance. "Smallest Size" Namespace optimized for smallest size. "Copy On Write" Namespace optimized for copy on write.
ValueMap | string | 0, 2, 3, 4, 5, .., 0x8000..0xFFFF
Values | string | Unknown, None, Best Performance, Smallest Size, Copy On Write, DMTF reserved, Vendor Reserved
ResourceType | uint16 |
Description | string | The type of resource this allocation setting represents. "Storage Volume" a logical block device. "Byte Addressable Persistent Memory" persistent memory accessible by load/store operations. "Block Addressable Persistent Memory" synthetic block device.
ModelCorrespondence | string | CIM_ResourceAllocationSettingData.OtherResourceType, CIM_ResourceAllocationSettingData.ResourceSubType
Override | string | ResourceType
ValueMap | string | 0, 1, 32, 35, 36, .., 0x8000..0xFFFF
Values | string | Unknown, Other, Storage Volume, Byte Addressable Persistent Memory, Block Addressable Persistent Memory, DMTF reserved, Vendor Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Address | string | CIM_ResourceAllocationSettingData
AddressOnParent | string | CIM_ResourceAllocationSettingData
AllocationUnits | string | CIM_ResourceAllocationSettingData
AutomaticAllocation | boolean | CIM_ResourceAllocationSettingData
AutomaticDeallocation | boolean | CIM_ResourceAllocationSettingData
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
ConsumerVisibility | uint16 | CIM_ResourceAllocationSettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
Limit | uint64 | CIM_ResourceAllocationSettingData
MappingBehavior | uint16 | CIM_ResourceAllocationSettingData
OtherResourceType | string | CIM_ResourceAllocationSettingData
Parent | string | CIM_ResourceAllocationSettingData
PoolID | string | CIM_ResourceAllocationSettingData
Reservation | uint64 | CIM_ResourceAllocationSettingData
ResourceSubType | string | CIM_ResourceAllocationSettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
VirtualQuantity | uint64 | CIM_ResourceAllocationSettingData
VirtualQuantityUnits | string | CIM_ResourceAllocationSettingData
Weight | uint32 | CIM_ResourceAllocationSettingData
ComponentSetting | string[] | CIM_SettingData
Connection | string[] | CIM_ResourceAllocationSettingData
HostResource | string[] | CIM_ResourceAllocationSettingData

## Class Methods