# Class CIM_StoragePoolDiagnosticSettingData
extends CIM_DiagnosticSettingData

This class defines the additional settings to be used for storage pool diagnostic tests.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_DiagnosticSettingData
|
+--CIM_StoragePoolDiagnosticSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines the additional settings to be used for storage pool diagnostic tests.
UMLPackagePath | string | CIM::Device::Storage
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Depth | uint16 |
Description | string | This property is used by a client to identify the depth of search for related components. The depth refers to the levels of indirection to reach a related element. If the test does not support the Depths setting, then this should be NULL. The possible non-values for depth include: * 0 - only test the pool * 1 - test one level removed from the pool * 2 - test two levels removed from the pool * 65535 - test all levels removed from the pool.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
HaltOnError | boolean | CIM_DiagnosticSettingData
InstanceID | string | CIM_SettingData
NonDestructive | boolean | CIM_DiagnosticSettingData
PercentOfTestCoverage | uint8 | CIM_DiagnosticSettingData
QueryTimeout | uint32 | CIM_DiagnosticSettingData
QuickMode | boolean | CIM_DiagnosticSettingData
ResultPersistence | uint32 | CIM_DiagnosticSettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData
LogOptions | uint16[] | CIM_DiagnosticSettingData
LogStorage | uint16[] | CIM_DiagnosticSettingData
LoopControl | uint16[] | CIM_DiagnosticSettingData
LoopControlParameter | string[] | CIM_DiagnosticSettingData
OtherLogOptionsDescriptions | string[] | CIM_DiagnosticSettingData
OtherLogStorageDescriptions | string[] | CIM_DiagnosticSettingData
OtherLoopControlDescriptions | string[] | CIM_DiagnosticSettingData
VerbosityLevel | uint16[] | CIM_DiagnosticSettingData

## Class Methods