# Class CIM_PrintJob
extends CIM_Job

Description of a print request that is either waiting on a Queue for a Printer to become available or in the process of being output on a Printer, or that has previously been printed on a Printer. PrintJobs are weak to their current Queue, or to the last Queue that held them. The ABNF for CIM references to PWG Standards and MIBs is in the directory 'ftp://ftp.pwg.org/pub/pwg/general/process' in the file 'pwg-cim-references-format-20060309.txt'. An example for a MappingStrings reference to a PWG Standard is 'PWG5101-1.PWG|Section 4 Media Color Names'. An example for a MappingStrings reference to a PWG MIB is 'MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorCompletedJobs'.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_Job
|
+--CIM_PrintJob

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Description of a print request that is either waiting on a Queue for a Printer to become available or in the process of being output on a Printer, or that has previously been printed on a Printer. PrintJobs are weak to their current Queue, or to the last Queue that held them. The ABNF for CIM references to PWG Standards and MIBs is in the directory 'ftp://ftp.pwg.org/pub/pwg/general/process' in the file 'pwg-cim-references-format-20060309.txt'. An example for a MappingStrings reference to a PWG Standard is 'PWG5101-1.PWG|Section 4 Media Color Names'. An example for a MappingStrings reference to a PWG MIB is 'MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorCompletedJobs'.
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.29.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CharSet | string |
Description | string | Specifies the character set and encoding method that should be used by the Printer for the management of this Job. The strings should conform to the semantics and syntax that are specified by section 4.1.2 'Charset parameter' in RFC 2046 (MIME Part 2) and contained in the IANA character-set registry. Examples include 'utf-8', 'us-ascii', and 'iso-8859-1'.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jobCodedCharSet, MIB.IETF|IANA-CHARSET-MIB.IANACharset, RFC2911.IETF|Job.attributes-charset
ModelCorrespondence | string | CIM_Printer.CharSetsSupported
Copies | uint32 |
Description | string | The number of physical copies of the output that will be produced from this Job.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jobCopiesRequested, RFC2911.IETF|Job.copies
ModelCorrespondence | string | CIM_Printer.MaxCopies
ElapsedTime | datetime |
Description | string | The processing elapsed time of this instance of PrintJob, after the Job has completed. Note: This property is NOT meaningful before PrintJob completion.
MappingStrings | string | RFC2911.IETF|Section 4.3.14.3 time-at-completed, RFC2911.IETF|Section 4.3.14.7 date-time-at-completed
ModelCorrespondence | string | CIM_PrintJob.TimeCompleted
Override | string | ElapsedTime
ElementName | string |
Description | string | The user-friendly name for this instance of PrintJob. In addition, the user-friendly name can be used as an index property for a search or query. (Note: The name does not have to be unique within a namespace.) This name shall be supplied by the client or generated by the PrintService (if missing in job creation operation).
MappingStrings | string | RFC2911.IETF|Section 4.3.5 job-name
Override | string | ElementName
Required | boolean | true
HorizontalResolution | uint32 |
Description | string | The resolution of the in Pixels per Inch for the Job in the cross-feed direction, i.e., short-edge in portrait feed mode.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.printerResolutionRequested, RFC2911.IETF|Job.printer-resolution
ModelCorrespondence | string | CIM_Printer.HorizontalResolution
PUnit | string | pixel / inch
Units | string | Pixels per Inch
JobID | string |
Description | string | Uniquely identifies this Job within its scoping Queue, but NOT across different Queues or PrintServices.
Key | boolean | true
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jmJobIndex, MIB.IETF|Job-Monitoring-MIB.jmJobSubmissionID, RFC2911.IETF|Job.job-id
JobOrigination | string |
Description | string | Provides additional information, beyond Job Owner that is inherited from CIM_Job, to identify the origins of the PrintJob. This property could include information such as the System, Application, or Process that created the Job.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jobOriginatingHost, MIB.IETF|Job-Monitoring-MIB.submittingServerName, MIB.IETF|Job-Monitoring-MIB.submittingApplicationName, RFC2911.IETF|Job.job-originating-user-name
JobSize | uint32 |
Description | string | Specifies the size of the PrintJob (as a byte stream) in units of Kbytes.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jmJobKOctetsProcessed, RFC2911.IETF|Job.job-k-octets
ModelCorrespondence | string | CIM_Printer.MaxSizeSupported, CIM_PrintQueue.MaxJobSize
PUnit | string | byte * 10^3
Units | string | KiloBytes
JobStatus | string |
Description | string | The inherited JobStatus is used to provide additional information about the status of a PrintJob beyond that enumerated by PrintJobStatus.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jmJobState, MIB.IETF|Job-Monitoring-MIB.jmJobStateReasons1, RFC2911.IETF|Job.job-state, RFC2911.IETF|Job.job-state-reasons, RFC2911.IETF|Job.job-state-message
ModelCorrespondence | string | CIM_PrintJob.PrintJobStatus
Override | string | JobStatus
Language | uint16 |
Deprecated | string | CIM_PrintJob.MimeTypes
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use MimeTypes. Enumerated print languages are only available in the IETF Printer MIB v1/v2 (RFC 1759/3805) and are not available in open standard print protocols (i.e., no known mapping). Deprecated description: Specifies the print language that is used by this Job. Note: For legacy compatiblity reasons, this property is NOT exactly aligned (in order of values) with the authoritative PrtInterpreterLangFamilyTC in the IANA Printer MIB, unlike the newer property PrintInterpreter.LangType (which is exactly aligned with the IANA Printer MIB).
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterLangFamily, MIB.IETF|IANA-PRINTER-MIB.PrtInterpreterLangFamilyTC, MIB.IETF|Job-Monitoring-MIB.documentFormat, PWG5100-7.PWG|Job.document-format-supplied
ModelCorrespondence | string | CIM_Printer.LanguagesSupported, CIM_PrintService.LanguagesSupported, CIM_PrintJob.MimeTypes
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, ..
Values | string | Other, Unknown, PCL, HPGL, PJL, PS, PSPrinter, IPDS, PPDS, EscapeP, Epson, DDIF, Interpress, ISO6429, Line Data, MODCA, REGIS, SCS, SPDL, TEK4014, PDS, IGP, CodeV, DSCDSE, WPS, LN03, CCITT, QUIC, CPAP, DecPPL, Simple Text, NPAP, DOC, imPress, Pinwriter, NPDL, NEC201PL, Automatic, Pages, LIPS, TIFF, Diagnostic, CaPSL, EXCL, LCDS, XES, MIME, TIPSI, Prescribe, LinePrinter, IDP, XJCL, PDF, RPDL, IntermecIPL, UBIFingerprint, UBIDirectProtocol, Fujitsu, PCLXL, ART, CGM, JPEG, CALS1, CALS2, NIRS, C4, XPS, OpenXPS, DMTF Reserved
NaturalLanguage | string |
Description | string | Identifies the language that should be used by the Printer for the management of this Job. The specified value should conform to RFC 5646. For example, 'en' is used for English.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jobNaturalLanguageTag, RFC2911.IETF|Job.attributes-natural-language
ModelCorrespondence | string | CIM_Printer.NaturalLanguagesSupported
NumberUp | uint32 |
Description | string | The number of print-stream pages that should be rendered onto a single media sheet when the Printer outputs this PrintJob.
MappingStrings | string | RFC2911.IETF|Job.number-up
ModelCorrespondence | string | CIM_Printer.MaxNumberUp
PrintJobStatus | uint16 |
Description | string | Describes the current state of this Job with respect to the PrintQueue and the Printer. Additional information can be specified in JobStatus. 1 (Other) means this Job is in some non-standard state. 2 (Unknown) means this Job is in an unknown state. 3 (Pending) maps to IPP job-state 'pending'. 4 (Blocked) maps to IPP job-state 'pending-held'. 5 (Completed) maps to IPP job-state 'completed'. 6 (Completed With Error) maps to IPP job-state 'completed' in combination with IPP job-state-reasons 'completed-with-errors'. 7 (Printing) maps to IPP job-state 'processing'. 8 (Processing Stopped) maps to IPP job-state 'processing-stopped'. 9 (Canceled) maps to IPP job-state 'canceled'. 10 (Aborted) maps to IPP job-state 'aborted'.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jmJobState, RFC2911.IETF|Job.job-state
ModelCorrespondence | string | CIM_PrintJob.TimeCompleted, CIM_PrintJob.JobStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | Other, Unknown, Pending, Blocked, Complete, Completed With Error, Printing, Processing Stopped, Canceled, Aborted
QueueCreationClassName | string |
Description | string | The CreationClassName of the scoping Queue.
Key | boolean | true
MaxLen | uint32 | 256
Propagated | string | CIM_PrintQueue.CreationClassName
QueueName | string |
Description | string | The Name of the scoping Queue.
Key | boolean | true
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jmGeneralJobSetName, MIB.IETF|Job-Monitoring-MIB.queueNameRequested, RFC2911.IETF|Job.output-device-assigned
MaxLen | uint32 | 256
Propagated | string | CIM_PrintQueue.Name
RequiredPaperType | string |
Description | string | A string that specifies the type of paper that is required by this PrintJob. The values of the property SHOULD conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property. See older Appendix B 'Media Size Names' and Appendix C 'Media Names' of IETF Printer MIB v2 [RFC3805] which list the values of standardized media names defined in ISO DPA [ISO10175].
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Job-Monitoring-MIB.mediumRequested, RFC2911.IETF|Job.media
ModelCorrespondence | string | CIM_Printer.PaperTypesAvailable, CIM_PrintService.PaperTypesAvailable
SchedulingInformation | string |
Deprecated | string | No value
Description | string | Note: The use of this free-form string property is deprecated in lieu of the more semantically rich CIM_JobSettingData class inherited from CIM_Job.
StartTime | datetime |
Description | string | The processing start time of this instance of PrintJob.
MappingStrings | string | RFC2911.IETF|Section 4.3.14.2 time-at-processing, RFC2911.IETF|Section 4.3.14.6 date-time-at-processing
Override | string | StartTime
SystemCreationClassName | string |
Description | string | The CreationClassName of the scoping System.
Key | boolean | true
MaxLen | uint32 | 256
Propagated | string | CIM_PrintQueue.SystemCreationClassName
SystemName | string |
Description | string | The Name of the scoping System.
Key | boolean | true
MappingStrings | string | MIB.IETF|SNMPv2-MIB.sysName
MaxLen | uint32 | 256
Propagated | string | CIM_PrintQueue.SystemName
TimeCompleted | datetime |
Description | string | The time when this Job was completed. This value is valid only if the PrintJobStatus has been assigned to 'Complete' or 'Completed With Error'.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.jobCompletionTime, RFC2911.IETF|Job.date-time-at-completed
ModelCorrespondence | string | CIM_PrintJob.PrintJobStatus
TimeSubmitted | datetime |
Description | string | The creation time of this instance of PrintJob.
MappingStrings | string | RFC2911.IETF|Section 4.3.14.1 time-at-creation, RFC2911.IETF|Section 4.3.14.5 date-time-at-creation
Override | string | TimeSubmitted
VerticalResolution | uint32 |
Description | string | The resolution in Pixels per Inch for the Job in the feed direction, i.e., long-edge in portrait feed mode.
MappingStrings | string | MIB.IETF|Job-Monitoring-MIB.printerResolutionRequested, RFC2911.IETF|Job.printer-resolution
ModelCorrespondence | string | CIM_Printer.VerticalResolution
PUnit | string | pixel / inch
Units | string | Pixels per Inch
Finishing | uint16[] |
ArrayType | string | Indexed
Description | string | Note: The use of this property will been deprecated due to ambiguity in a future version. Instead use the experimental property Finishings. Enumerated finishings are not available in open standard print protocols (i.e., no known mapping). Deprecated description: An array of integers that indicates the type of finishing that is required by this Job. It is equivalent to the Capabilities property that is provided by the Printer.
ModelCorrespondence | string | CIM_Printer.Capabilities, CIM_PrintService.Capabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21
Values | string | Unknown, Other, Color Printing, Duplex Printing, Copies, Collation, Stapling, Transparency Printing, Punch, Cover, Bind, Black and White Printing, One Sided, Two Sided Long Edge, Two Sided Short Edge, Portrait, Landscape, Reverse Portrait, Reverse Landscape, Quality High, Quality Normal, Quality Low
MimeTypes | string[] |
Description | string | Specifies the MIME types that are used by the PrintJob.
ModelCorrespondence | string | CIM_PrintJob.Language, CIM_Printer.MimeTypesSupported, CIM_PrintService.MimeTypesSupported
RequiredJobSheets | string[] |
Description | string | Describes the job sheets that should be used when this Job is output on the Printer. Complete standard values are in the IANA IPP Registry. Additional vendor or site values may also be used. Standard values defined in IPP/1.1 (RFC 2911) include: Value 'none' indicates no job start/end sheets. Value 'standard' indicates one or more site-specific standard job sheets.
MappingStrings | string | RFC2911.IETF|Job.job-sheets
ModelCorrespondence | string | CIM_Printer.AvailableJobSheets

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
DeleteOnCompletion | boolean
Description | string
DetailedStatus | uint16
ErrorCode | uint16
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
JobRunTimes | uint32
LocalOrUtcTime | uint16
Name | string
Notify | string
OperatingStatus | uint16
OtherRecoveryAction | string
Owner | string
PercentComplete | uint16
PrimaryStatus | uint16
Priority | uint32
RecoveryAction | uint16
RunDay | sint8
RunDayOfWeek | sint8
RunMonth | uint8
RunStartInterval | datetime
ScheduledStartTime | datetime
Status | string
UntilTime | datetime
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
KillJob | uint32