# Class CIM_MemoryMappedIO
extends CIM_SystemResource

Personal Computer architecture Memory Mapped I/O. This class addresses both memory and port I/O resources. The property, MappedResource, defines whether memory or I/O is mapped (and for I/O whether the mapping is to a memory or a port space).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_SystemResource
|
+--CIM_MemoryMappedIO

## Direct Known Subclasses

CIM_MemoryResource
CIM_PortResource

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Personal Computer architecture Memory Mapped I/O. This class addresses both memory and port I/O resources. The property, MappedResource, defines whether memory or I/O is mapped (and for I/O whether the mapping is to a memory or a port space).
UMLPackagePath | string | CIM::System::SystemResources
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CreationClassName | string |
Description | string | CreationClassName indicates the name of the class or the subclass used in the creation of an instance. When used with the other key properties of this class, this property allows all instances of this class and its subclasses to be uniquely identified.
Key | boolean | true
MaxLen | uint32 | 256
CSCreationClassName | string |
Description | string | The scoping ComputerSystem's CreationClassName.
Key | boolean | true
MaxLen | uint32 | 256
Propagated | string | CIM_ComputerSystem.CreationClassName
CSName | string |
Description | string | The scoping ComputerSystem's Name.
Key | boolean | true
MaxLen | uint32 | 256
Propagated | string | CIM_ComputerSystem.Name
EndingAddress | uint64 |
Description | string | Ending address of memory mapped I/O.
MappingStrings | string | MIF.DMTF|Memory Mapped I/O|001.2
MappedResource | uint16 |
Description | string | Type of memory mapped I/O. MappedResource defines whether memory or I/O is mapped, and for I/O, whether the mapping is to a memory or a port space.
ValueMap | string | 0, 1, 2, 3
Values | string | Other, Mapped Memory, I/O Mapped to Memory Space, I/O Mapped to Port Space
StartingAddress | uint64 |
Description | string | A part of the object's key value, the starting address of memory mapped I/O.
Key | boolean | true
MappingStrings | string | MIF.DMTF|Memory Mapped I/O|001.1

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
ImplementationInfo | uint16
InstallDate | datetime
InstanceID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryStatus | uint16
RequestedState | uint16
Shareable | boolean
Status | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
RequestStateChange | uint32