# Class CIM_WBEMServer
extends CIM_Service

CIM_WBEMServer represents a WBEMServer and serves as an aggregation point for the WBEM Server settings, capabilities, services, protocols, etc.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_WBEMServer

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_WBEMServer represents a WBEMServer and serves as an aggregation point for the WBEM Server settings, capabilities, services, protocols, etc.
UMLPackagePath | string | CIM::Interop::WBEMServer
Version | string | 2.38.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Description | string |
Description | string | The Description of the WBEM Server (e.g. ACME WBEM Server 1.0.0).
Override | string | Description
Required | boolean | true
ElementName | string |
Description | string | The ElementName property is used as a name of the WBEM Server for human interfaces. For example, "ACME WBEM Server").
Override | string | ElementName
Required | boolean | true
Name | string |
Description | string | The Name property is used to uniquely identify a WBEM Server. The WBEM Server shall ensure that this value is globally unique.
Key | boolean | true
MaxLen | uint32 | 256
Override | string | Name

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
DetailedStatus | uint16
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32