# Class CIM_StoragePoolDiagnosticSettingData
extends CIM_DiagnosticSettingData

This class defines the additional settings to be used for storage pool diagnostic tests.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_DiagnosticSettingData
|
+--CIM_StoragePoolDiagnosticSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines the additional settings to be used for storage pool diagnostic tests.
UMLPackagePath | string | CIM::Device::Storage
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Depth | uint16 |
Description | string | This property is used by a client to identify the depth of search for related components. The depth refers to the levels of indirection to reach a related element. If the test does not support the Depths setting, then this should be NULL. The possible non-values for depth include: * 0 - only test the pool * 1 - test one level removed from the pool * 2 - test two levels removed from the pool * 65535 - test all levels removed from the pool.

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
ChangeableType | uint16
ConfigurationName | string
Description | string
ElementName | string
Generation | uint64
HaltOnError | boolean
InstanceID | string
NonDestructive | boolean
PercentOfTestCoverage | uint8
QueryTimeout | uint32
QuickMode | boolean
ResultPersistence | uint32
SoID | string
SoOrgID | string
ComponentSetting | string[]
LogOptions | uint16[]
LogStorage | uint16[]
LoopControl | uint16[]
LoopControlParameter | string[]
OtherLogOptionsDescriptions | string[]
OtherLogStorageDescriptions | string[]
OtherLoopControlDescriptions | string[]
VerbosityLevel | uint16[]

## Class Methods