# Class CIM_ProcessorCore
extends CIM_EnabledLogicalElement

The CIM_ProcessorCore class inherits from CIM_EnabledLogicalElement and describes a specific processor core. CIM_ProcessorCore instances are related to the instance of CIM_Processor that represents the processor they are contained in.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ProcessorCore

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The CIM_ProcessorCore class inherits from CIM_EnabledLogicalElement and describes a specific processor core. CIM_ProcessorCore instances are related to the instance of CIM_Processor that represents the processor they are contained in.
UMLPackagePath | string | CIM::Device::Processor
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CoreEnabledState | uint16 |
Description | string | The CoreEnabledState property is the configuration state of the processor core. For example, the core might be disabled by the user (value=2), or disabled due to a POST error (value=3).
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, DMTF Reserved, Core Enabled, Core Disabled, Core Disabled by User, Core Disabled By POST Error)
InstanceID | string |
Description | string | Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. In order to ensure uniqueness within the NameSpace, the value of InstanceID SHOULD be constructed using the following 'preferred' algorithm: <OrgID>:<LocalID> Where <OrgID> and <LocalID> are separated by a colon ':', and where <OrgID> MUST include a copyrighted, trademarked or otherwise unique name that is owned by the business entity creating/defining the InstanceID, or is a registered ID that is assigned to the business entity by a recognized global authority (This is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness <OrgID> MUST NOT contain a colon (':'). When using this algorithm, the first colon to appear in InstanceID MUST appear between <OrgID> and <LocalID>. <LocalID> is chosen by the business entity and SHOULD not be re-used to identify different underlying (real-world) elements. If the above 'preferred' algorithm is not used, the defining entity MUST assure that the resultant InstanceID is not re-used across any InstanceIDs produced by this or other providers for this instance's NameSpace. For DMTF defined instances, the 'preferred' algorithm MUST be used with the <OrgID> set to 'CIM'.
Key | boolean | true
Override | string | InstanceID
LoadPercentage | uint16 |
Description | string | Loading of this processor core, averaged over the last minute, in Percent.
Gauge | boolean | true
PUnit | string | percent
Units | string | Percent

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryStatus | uint16
RequestedState | uint16
Status | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
RequestStateChange | uint32