# Class CIM_AdminDomain
extends CIM_System

This is a special grouping of ManagedSystemElements. The grouping is viewed as a single entity, reflecting that all of its components are administered similarly, either by the same user, group of users, or policy. It serves as an aggregation point to associate one or more of the following elements: network devices, such as routers and switches, servers, and other resources that can be accessed by end systems. This grouping of devices plays an essential role in ensuring that the same administrative policy and actions are applied to all of the devices in the grouping. The specific behavior and/or semantics of the AdminDomain can be identified through its aggregated and associated entities.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_System
|
+--CIM_AdminDomain

## Direct Known Subclasses

CIM_AutonomousSystem
CIM_J2eeDomain
CIM_Network
CIM_PolicyRepository
CIM_ReusablePolicyContainer
CIM_RoutingProtocolDomain
CIM_TierDomain

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This is a special grouping of ManagedSystemElements. The grouping is viewed as a single entity, reflecting that all of its components are administered similarly, either by the same user, group of users, or policy. It serves as an aggregation point to associate one or more of the following elements: network devices, such as routers and switches, servers, and other resources that can be accessed by end systems. This grouping of devices plays an essential role in ensuring that the same administrative policy and actions are applied to all of the devices in the grouping. The specific behavior and/or semantics of the AdminDomain can be identified through its aggregated and associated entities.
UMLPackagePath | string | CIM::Core::CoreElements
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
NameFormat | string |
Description | string | The NameFormat property identifies how the Name of the AdminDomain is generated, using the heuristic specified in the CIM V2 System Model specification. The property assumes that to determine and assign a Name the documented rules are traversed in order. The NameFormat Values list defines the precedence order for assigning the Name of the AdminDomain. "FC" has been deprecated and replaced by "WWN" to be consistent with the other ValueMaps.
MaxLen | uint32 | 64
ModelCorrespondence | string | CIM_AdminDomain.Name
Override | string | NameFormat
ValueMap | string | Other, AS, NAP, NOC, POP, RNP, IP, IPX, SNA, Dial, WAN, LAN, ISDN, Frame Relay, ATM, E.164, IB, FC, Policy Repository, WWN
Values | string | Other, Autonomous System, Network Access Provider, Network Operations Center, Point of Presence, Regional Network Provider, IP, IPX, SNA, Dial, WAN, LAN, ISDN, Frame Relay, ATM, E.164, Infiniband, Fibre Channel, Policy Repository, Fibre Channel Worldwide Name

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Status | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
Roles | string[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
RequestStateChange | uint32