# Class CIM_DeviceIdentity
extends CIM_LogicalIdentity

CIM_DeviceIdentity indicates that two LogicalDevices represent different aspects of the same underlying entity. This association refines the CIM_LogicalIdentity superclass by restricting it to the Device level and defining its use in well understood scenarios. One of these scenarios is to represent that a Device is both a 'bus' entity and a 'functional' entity. For example, a Device could be both a PCI Device (or a USB Device), as well as a CIM_Keyboard. The other scenario is where a Device plays multiple functional roles that can not be distinguished by their hardware realization alone. For example, a Fibre Channel adapter might have aspects of both a NetworkAdapter and a SCSIController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_LogicalIdentity
|
+--CIM_DeviceIdentity

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | CIM_DeviceIdentity indicates that two LogicalDevices represent different aspects of the same underlying entity. This association refines the CIM_LogicalIdentity superclass by restricting it to the Device level and defining its use in well understood scenarios. One of these scenarios is to represent that a Device is both a 'bus' entity and a 'functional' entity. For example, a Device could be both a PCI Device (or a USB Device), as well as a CIM_Keyboard. The other scenario is where a Device plays multiple functional roles that can not be distinguished by their hardware realization alone. For example, a Fibre Channel adapter might have aspects of both a NetworkAdapter and a SCSIController.
UMLPackagePath | string | CIM::Device::DeviceElements
Version | string | 2.6.0

## Class Properties

### Association References

Name | Reference Class
--- | ---
SameElement | CIM_LogicalDevice
SystemElement | CIM_LogicalDevice

## Class Methods