# Class CIM_ParticipatingCS
extends CIM_Dependency

A Cluster is composed of two or more ComputerSystems, operating together. A ComputerSystem may participate in multiple Clusters. When first establishing or bringing up a Cluster, only one ComputerSystem may be defined as participating in it. Therfore, the cardinality of the association for the ComputerSystem reference is Min (1). The use of this association is deprecated in lieu of using MemberOfCollection to RedundancySet.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_ParticipatingCS

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Deprecated | string | CIM_MemberOfCollection
Description | string | A Cluster is composed of two or more ComputerSystems, operating together. A ComputerSystem may participate in multiple Clusters. When first establishing or bringing up a Cluster, only one ComputerSystem may be defined as participating in it. Therfore, the cardinality of the association for the ComputerSystem reference is Min (1). The use of this association is deprecated in lieu of using MemberOfCollection to RedundancySet.
UMLPackagePath | string | CIM::System::SystemElements
Version | string | 2.54.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
RoleOfNode | uint16 |
Deprecated | string | CIM_ComputerSystem.Roles
Description | string | RoleOfNode indicates whether the Cluster nodes are peers (value = 2), connected in a master-slave/primary- secondary relationship (values = 3 for primary, 4 for secondary), available in a standby configuration (5) or of some other (1) or unknown (0) relationship. In a System/390 environment, the nodes are identified as "Base Plex" (value=6) or "Enhanced Plex" (value=7).
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7
Values | string | Unknown, Other, Peer, Primary, Secondary, Standby, Base Plex, Enhanced Plex
StateOfNode | uint16 |
Deprecated | string | CIM_ComputerSystem.EnabledState, CIM_ComputerSystem.OperationalStatus
Description | string | StateOfNode indicates the condition of the participating ComputerSystem in the Cluster. For example, one value is "Joining" (2).
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Joining, Paused, Available, Unavailable, Degraded

### Association References

Name | Reference Class
--- | ---
Antecedent | CIM_ComputerSystem
Dependent | CIM_Cluster

## Class Methods