# Class CIM_DeviceSAPImplementation
extends CIM_Dependency

An association between a ServiceAccessPoint (SAP) and how it is implemented. The cardinality of this association is many-to-many. A SAP can be provided by more than one LogicalDevice, operating in conjunction. And, any Device can provide more than one ServiceAccessPoint. When many LogicalDevices are associated with a single SAP, it is assumed that these elements operate in conjunction to provide the AccessPoint. If different implementations of a SAP exist, each of these implementations would result in individual instantiations of the ServiceAccessPoint object. These individual instantiations would then have associations to the unique implementations.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_DeviceSAPImplementation

## Direct Known Subclasses

CIM_PortImplementsEndpoint

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | An association between a ServiceAccessPoint (SAP) and how it is implemented. The cardinality of this association is many-to-many. A SAP can be provided by more than one LogicalDevice, operating in conjunction. And, any Device can provide more than one ServiceAccessPoint. When many LogicalDevices are associated with a single SAP, it is assumed that these elements operate in conjunction to provide the AccessPoint. If different implementations of a SAP exist, each of these implementations would result in individual instantiations of the ServiceAccessPoint object. These individual instantiations would then have associations to the unique implementations.
UMLPackagePath | string | CIM::Core::Device
Version | string | 2.10.0

## Class Properties

### Association References

Name | Reference Class
--- | ---
Antecedent | CIM_LogicalDevice
Dependent | CIM_ServiceAccessPoint

## Class Methods