# Class CIM_IPsecTransportAction
extends CIM_IPsecAction

IPsecTransportAction is used to specify that a transport-mode SA should be negotiated.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Policy
|
+--CIM_PolicyAction
|
+--CIM_SAAction
|
+--CIM_SANegotiationAction
|
+--CIM_IPsecAction
|
+--CIM_IPsecTransportAction

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | IPsecTransportAction is used to specify that a transport-mode SA should be negotiated.
MappingStrings | string | IPSP Policy Model.IETF|IPsecTransportAction
UMLPackagePath | string | CIM::IPsecPolicy
Version | string | 2.8.0

## Class Properties

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommonName | string
CreationClassName | string
Description | string
DoActionLogging | boolean
DoPacketLogging | boolean
ElementName | string
Generation | uint64
Granularity | uint16
GroupId | uint16
IdleDurationSeconds | uint64
InstanceID | string
MinLifetimeKilobytes | uint64
MinLifetimeSeconds | uint64
OtherGranularity | string
PolicyActionName | string
PolicyRuleCreationClassName | string
PolicyRuleName | string
SystemCreationClassName | string
SystemName | string
UsePFS | boolean
UsePhase1Group | boolean
VendorID | string
PolicyKeywords | string[]

## Class Methods