# Class CIM_ExtraCapacityGroup
extends CIM_RedundancyGroup

A class derived from RedundancyGroup indicating that the aggregated elements have more capacity or capability than is needed. An example of this type of redundancy is the installation of N+1 power supplies or fans in a system. The use of this class is being deprecated in lieu of using RedundancySet.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_RedundancyGroup
|
+--CIM_ExtraCapacityGroup

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_RedundancySet
Description | string | A class derived from RedundancyGroup indicating that the aggregated elements have more capacity or capability than is needed. An example of this type of redundancy is the installation of N+1 power supplies or fans in a system. The use of this class is being deprecated in lieu of using RedundancySet.
UMLPackagePath | string | CIM::Core::Redundancy
Version | string | 2.21.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LoadBalancedGroup | boolean |
Deprecated | string | CIM_RedundancySet.TypeOfSet
Description | string | Boolean indicating whether load balancing is supported by the ExtraCapacityGroup.
MinNumberNeeded | uint32 |
Deprecated | string | CIM_RedundancySet.MinNumberNeeded
Description | string | MinNumberNeeded indicates the smallest number of elements that must be operational in order to have redundancy. For example, in an N+1 redundancy relationship, the MinNumberNeeded property should be set equal to N.

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
OperatingStatus | uint16
PrimaryStatus | uint16
RedundancyStatus | uint16
Status | string
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods